# MULTI_QI

To optimize network performance, most remote activation functions take an array of MULTI_QI structures rather than just a single IID as input and a single pointer to the requested interface on the object as output, as do local machine activation functions. This allows a set of pointers to interfaces to be returned from the same object in a single round-trip to the server. In network scenarios, requesting multiple interfaces at the time of object construction can save considerable time over using a number of calls to the QueryInterface method for unique interfaces, each of which would require a round-trip to the server.

    typedef struct _MULTI_QI {
            const IID*    pIID;
            IUnknown *    pItf;
            HRESULT       hr;
        } MULTI_QI;

Members

pIID
  [in] Pointer to an interface identifier.
pItf
  [out] Pointer to the interface requested in pIID. Must be set to NULL on entry.
hr
  [out] Return value of the QueryInterface call made to satisfy the request for the interface requested in pIID. Common return values are S_OK and E_NOINTERFACE. Must be set to zero on entry.

See Also

CoGetInstanceFromFile, CoGetInstanceFromIStorage, CoCreateInstanceEx